Marlin WebUI by atbox.tech 

Disconnected

Status

Printer status

Printing status

Idle

Printing timer

Remain: 0:45:12

Estimated: 1:12:34

Elapsed: 0:00:00

Printing progress:

10%

1 of 123456

Temperatures

Auto temperature detection

1 sec 5 sec 10 sec 30 sec 60 sec

|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| Sensor   |  | | --- | | Hotend (extruder) sensor | | Bed sensor | | Detected   |  | | --- | | - | | - | | Set   |  | | --- | | - | | - | | Unit   |  | | --- | | - | | - | | Chart display   |  | | --- | | Show | | Show | |

Hotend fan speed

|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| |  |  | | --- | --- | | Current fan speed | - | | Set fan speed | - | | |  |  |  |  |  |  |  |  |  |  |  | | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | | OFF | 10% | 20% | 30% | 40% | 50% | 60% | 70% | 80% | 90% | FULL | | | |  | | |  |

Controls

Home positioning

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| All axis |  | X axis |  | Y axis |  | Z axis |
|  |  |  |  |  |  |  |

Movements

Steps movements size (mm)

Move on X axis

Move on Y axis

Move on Z axis

Steppers locking

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| Lock/Unlock all steppers (X, Y, Z, E) | | | | | |  |
| X stepper |  | Y stepper |  | Z stepper |  | E stepper |
|  |  |  |  |  |  |  |

Filament

File management

Upload...

Choose file

Upload

|  |  |  |
| --- | --- | --- |
| Filename (DOS8 Format)  - | File size  - | GCode Lines  - |

File processing

|  |  |
| --- | --- |
|  | Cancel Process |

SD Content management

Get content

SD Init SD Release

Selected file:

Files:

0

Folders:

0

SD File list

Console

0

G-Code command:

Send

GCode checksum value:

Console output:

Clear list

Save..

Info... ×

Marlin WebUI

Release date: January, 1 2020

Github project: [E4d-box-project](https://github.com/exilaus/E4d-box-project)

Facebook: [E4d@box](https://www.facebook.com/groups/372792116726814/about/)

Open source dependencies:

* [Marlin firmware](https://marlinfw.org/)
* [JQuery 3.5.1 (slim version)](https://jquery.com/)
* [Bootstrap v4.5.0](https://getbootstrap.com/)
* [Bootstrap4 toggle switch v3.6.1](https://gitbrent.github.io/bootstrap4-toggle/)
* [Fontastic](http://fontastic.me/)
* [Chart.js](https://www.chartjs.org/)
* [FileSaver.js](https://github.com/eligrey/FileSaver.js)

Close

Settings.. ×

* Auto connect:If ON the application will try to connect automatically on start
* Temp interval:  
  1 sec 5 sec 10 sec 30 sec 60 secSet the default temperature detection interval (secs)
* Temp unit:  
  Celsius (default) Fahrenheit KelvinSet the default temperature unit
* Default panel:  
  Console Controls Status (default) Temperature UploadSet the default shown panel on start
* Trace direction:  
  Append PrependSet the console trace direction
* Trace symbol  
  Icon Letter  
  Chevron: U/D Chevron: L/R Arrow: U/D Arrow: L/RSet the console message direction symbol
* Logging level  
  Info (default) Warning Error Debug VerboseSet the JavaScript logging level

Settings saved successfully

Close

Save

GCommand presets ×

* Replace {N} chars with the specific parameter that you need if present (ie: G1 X{0} => G1 X10)

Close

Connect... ×

Ooopsss!

Marlin firmware Web Socket is not connected.

Would you like connect it now?

Cancel

Connect now

Deletion confirmation ×

Are you sure to delete

SD card file?

This operation cannot be undone.

File deleted successfully

No

Yes

Print confirmation ×

Are you sure to start printing of

Printing started successfully

No

Yes

Message ×

OK